BARODA U.P. BANK

REGIONAL OFFICE AMETHI

(Sponsored by Bank of Baroda)

(INTERIOR FURNISHING VENDORS EMPANELLED WITH

BARODA U.P. BANK REGIONAL OFFICE, AMETHI CAN APPLY)

BARODA U.P. BANK

Regional Office AMETHI

Near Piyush Petrol Pump Raebareli to Sultanpur Road

Gauriganj Amethi, 227409

TENDER FOR INTERIOR FURNISHING WORK

AT

MUSAFIRKHANA BRANCH

DISTT. AMETHI

# Architects

**M/s Mohit & Associates,**

**L-2/554 Vineet Khand, Gomti Nagar,**

**Lucknow**

**Ph – 9582218092, 7428217659**

BARODA U.P. BANK

REGIONAL OFFICE AMETHI

(Sponsored by Bank of Baroda)

BARODA U.P. BANK

Regional Office AMETHI

Near Piyush Petrol Pump Raebareli to Sultanpur Road

Gauriganj Amethi, 227409

---------------------------------------------------------------------------------------------------------------------

**Subject: Interior Furnishing WORK for**

**Baroda U.P. Bank at MUSAFIRKHANA Branch,**

**Distt. AMETHI**

ISSUE OF TENDERS FROM 04.05.2022 TO 19.05.2022

LAST DATE OF SUBMISSION 19.05.2022 up to 3.00 pm

TENDER OPENING DATE 19.05.2022 TIME 4.30 PM

(TENDERS WILL BE OPENED IN PRESENCE OF CONTRACTING AGENCIES OR THEIR AUTHORISED REPRESENTATIVES)

TENDERS CAN BE DOWNLOADED FROM THE BANK’S WEBSITE www.barodagraminbank.com OR CAN BE COLLECTED FROM THE FOLLOWING ADDRESS AND SHOULD BE SUBMITTED BY GIVEN DATE ALONG WITH NON RETURNABLE TENDER DOCUMENT FEES OF Rs. 500/- BY WAY OF DEMAND DRAFT IN FAVOUR OF BARODA U.P. BANK AND PAYABLE AT GAURIGANJ AMETHI. (Only Our Bank Empanelled Furnishers Can Apply)

PLACE OF TENDER COLLECTION / SUBMISSION:

BARODA U.P. BANK

Regional Office AMETHI

Near Piyush Petrol Pump Raebareli to Sultanpur Road

Gauriganj Amethi, 227409

TENDER ISSUED TO: M/S\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

NOTICE FOR INTIMATION TENDER

To,

M/s.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Dear Sir,

**Sub: - Interior Furnishing for Baroda U.P. Bank at MUSAFIRKHANA Branch, Distt. AMETHI**

1) Sealed, item rate, tenders are invited in the prescribed format from experienced contractors empanelled for carrying out jobs in AMETHI Region for execution of Interior Furnishing work for Baroda U.P. Bank at MUSAFIRKHANA Branch Distt. AMETHI. As per following details:

**Name of the work : Interior Furnishing works for Baroda U.P. Bank at MUSAFIRKHANA Branch Distt. AMETHI**

Earnest Money Deposit : Rs. 5000/- (Rs. Five Thousands Only)

by Demand draft / Pay Order payable at AMETHI

& drawn in favor of BARODA U.P. BANK

Period of Completion : 4 (FOUR) weeks

Validity of Tender : 120 days

Date of Issue of Tender : From 04.05.2022 on any working day during Office hours

Tender Cost : Rs. 500/-(Rs. Five Hundred Only) Applicable only in

demand draft collection of hard copy   of tender from our office.

Last date of submission of : Up to 3.00 p.m. on 19.05.2022 .

Tender

Date & Time of opening the : 4.30 p.m. on 19.05.2022

Tender

2) The tender document can be downloaded from our bank’s website www.barodagraminbank.com or obtained from the Office of the Regional Manager, Baroda U.P. Bank, Regional Office AMETHI Near Piyush Petrol Pump Raebareli to Sultanpur Road Gauriganj Amethi, 227409 and should be submitted in original, dully stamped, and sealed in the same office with requisite tender fees.

3) The item rates under the contract include for full, final & entire completion of all works in all respects described in contract & as shown in drawings forming part of the contract. Contractor must quote item rates for all the items of work. Tenders will be opened in the presence of contracting agencies or their authorized representatives.

4) The tenders shall be submitted in a sealed envelope. The envelope shall be marked as Technical Bid, shall contain Volume- 1 of the tender, EMD in the form of Demand Draft / Pay Order and any other matter.

5) The Envelope of the contractors who have complied with the required EMD will be opened on the due date & time of opening.

6) Tenders are to be submitted in a sealed envelope cover super scribed “Tender for Interior Furnishing for Baroda U.P. Bank at MUSAFIRKHANA Branch, Distt. AMETHI.

7) The tenderer must use only the tender forms issued for the purpose to fill in the rates intimation of tender quoted by letter, telegram / telex will not be acceptable.

8) Tenderers are advised not to make any alternation / modification in the tender documents, item of work or in any respect whatsoever. Violation of this requirement will make the Tender Liable for rejection.

9) In case of postal delivery, the tenderer has to ensure that tender is reached before the due date and time. The bank will not be responsible for damage in the transit and delay of receipt to tender, if any or sent by a special messenger. Tender received late shall be rejected.

10) Every page of the tender documents should be signed by the person or persons submitting the tender in token of his / their having acquainted himself / themselves with the General and Special Conditions of Contract, Specifications etc., as laid down. Any tender with any of the documents not so signed will be subjected to rejection.

11) No consideration will be given to a tender received after the time stipulated above and no extension will be allowed for submission of the tender. The Baroda U.P. Bank shall not be bound to accept the lowest tender and reserves the right to accept or reject any or all the tenders without assigning any reason whatsoever.

12) This notice inviting tenders, the conditions of tender and the duly completed form of tender etc. will form part of the Agreement to be executed by the successful tenderer with the bank.

The following document forming a part of tender are enclosed herewith

1. Introduction
2. Tender Notice
3. Special Instructions & Conditions
4. Letter of Offer
5. Form of Agreement
6. Preamble to B.O.Q.
7. Mode of Measurement
8. List of Approved Manufacturers for Materials
9. Bill of Quantities

This tender notice shall form part of the contract and non-submission of tender in the above manner will render your offer liable for rejection.

FOR Baroda U.P. Bank

CHIEF MANAGER

Terms & Conditions for Vendors:-

1. Advance is not right of Vendor. The rights of advance to Vendor solely rests with Bank.
2. Any request of advance from Vendor will only be entertained if work order is of more than Rs. 10.00 Lakhs
3. Only Vendor having valid & active e-mail id should participate in Tender process.
4. Work order sent via e-mail will be considered accepted if there is no response within 3 days of e-mail sent from Regional/ Circle office.
5. Day to day communication/ instructions will be via e-mail and Vendor should be prompt in replying to every e-mail sent by Regional Office/ Circle office / Architect etc.
6. Quantity of any item can be modified at the time of furnishing as per need of the branch.
7. Vendor has to strictly provide items of make as per list attached on page no 18,19 & 20.

Bank reserves the right to cancel the work order without any payment if quality of items are not as per list provided.

#### 

#### TENDER NOTICE

**Subject: Interior Furnishing work for Baroda U.P. Bank at MUSAFIRKHANA Branch Distt. AMETHI**

Sealed item rate tenders are invited by M/s Baroda U.P. Bank,The REGIONAL HEAD , BUPB Bank, Regional Office, Near Piyush Petrol Pump Raebareli to Sultanpur Road Gauriganj Amethi, 227409

The work to be completed within 4 weeks from 3rd days of the date of acceptance of work order placed by M/s Baroda U.P. Bank.

The tenderers are required to complete form of tender, price the schedule of quantities and sign each page of tender documents before submission. The completed set is to be enclosed in a sealed envelope addressed to:

Regional Head Baroda U.P. Bank , Regional Office, Near Piyush Petrol Pump Raebareli to Sultanpur Road Gauriganj Amethi, 227409.

1. Tenders will be received up to 19.05.2022 on **15.00 hrs.**
2. No tender will be received after the expiry of the time notified for receiving tenders under any circumstances whatsoever.
3. The tender will be opened at **16.30** hours on 19.05.2022 at above address in the presence of authorized representatives contracting agencies.
4. Tender shall remain valid for acceptance for a period of 90 days from the notified last date of tender submission.
5. The Bank reserves the right to reject any or all tender received without assignment of any reasons thereof.
6. The tender rate against each item of work / price indicated in the schedule of quantities and rates / price should be indicated both in words and figures. In case of any discrepancy, the rates indicated in words would prevail.
7. The rates quoted against each item of work / price should be for the complete finished item of work and include all labour, material, taxes, overhead, duties, etc. Any statutory change in the tax structure after opening of the tender shall be reimbursed by the Bank as per actual.
8. Each tender shall be accompanied by Earnest Money of **Rs. 5,000/-** **(Rs. Five Thousand Only)** in the form of Pay Order / Demand Draft in favour of **Baroda U.P. Bank,** payable at **GAURIGANJ** **AMETHI**. Tenders without Earnest Money shall be summarily rejected.
9. The earnest money deposited shall not carry any interest and will be refunded to the unsuccessful tenderers. Earnest money paid by the successful contractor will be retained by the Bank till completion of the work.

1. Earnest money paid by contractor shall be forfeited by the Bank if contractor fails to undertake the job if he is communicated about acceptance of his rates.
2. All tenders in whom any of the prescribed conditions are not fulfilled or incomplete in any respect are liable to be rejected. This tender notice shall form part of the contract documents.

**GENERAL CONDITIONS OF CONTRACT**

**Subject: Interior Furnishing work for Baroda U.P. Bank at MUSAFIRKHANA Branch Distt. AMETHI.**

## General Instructions to Contractor

|  |
| --- |
| **Inspection of sites**: The contractor shall visit and examine the site and satisfy as to the nature and correct dimensions of work and facilities for obtaining material and shall obtain generally his own information on all matters affecting the execution of work. No extra charge made in consequence of any misunderstanding or incorrect information on any of these points on the ground of insufficient description will be allowed. All expenses incurred by the contractors in connection with obtaining information for submitting this tender including his visit to site and efforts in compiling the tender shall be borne by the tenderer ad no claims for reimbursement thereof shall be entertained. |
|  |
| **Safety Regulations:** The contractor shall take all the necessary precautions while working and to safeguard adjacent property, Bank’s property, Bank’s employees, and traffic persons |
|  |
| **Compliance to local laws**: The contractor shall conform to the provisions of any Act of the Legislature relating to the work and to the Regulation of Bye Laws of any authority. He shall also obtain the permission of the Municipality or any other Authorities if required under the existing rules. |
| **Site cleaning:** All the rates quoted are inclusive of removal of rubbish / debris collected during the progress of work, rejected material and clearance of site before and after the work is completed. Not more than one truck load shall be stored that to for not more than 3 days. The contractor shall arrange to remove the same immediately. If the contractor is failing to remove the same and the expenses shall be recovered from the contractor and he will not dispute for the expenses so incurred. |
|  |
| **Vouchers / bills**: Contractor shall upon the request of the Bank furnish bills, invoices, accounts, receipts and other vouchers for all materials brought on site to prove that the material purchased are as mentioned in the specification. |
|  |
| **Contractor’s responsibility**: The work will from time to time be examined by Project Architect, but such examination shall not in any way exonerate the contractor from the obligation to remedying any defects which may be observed at any stage of the work or after the same is completed. |
|  |
| Dismissal from work: The contractor shall upon the written request of the Project Architect immediately dismiss from the work any person employed by him thereon, who may in the opinion of the authority be incompetent or misconduct himself and such person shall not be again employed on the work, without the permission of the bank. |
|  |
| Order of work, etc.: Bank reserves the right to fix the order in which the various items of work involved are to be executed. However, the contractor shall be responsible for the completion of the entire job within the item limit specified failing which liquidated damages as mentioned in clause No.49 shall be recovered from the contractor. |
| **Commencement of work**: The work must be started within **3rd days** upon accepting the work order and the program me for carrying out the various jobs shall be drawn out in consultation with the Project Architect. Adequate labour force shall be provided to complete the work within the specified period. Proper security aspects should be taken care of by adequate vigilance in view of the importance of the building. Default in compliance with the programmes so finalized shall entail operation of liquidated damages as stated. |
| **Subletting the work**: The contractor shall not directly or indirectly sublet the work to other party without written permission from the bank. |
|  |
| **Quantities of works are provisional**: The quantities mentioned in schedule are provisional and likely to increase / decrease to any extent or may be omitted thus altering the aggregate value of the contract. No claim for loss of profit / business shall be entertained on this account. |
|  |
| **Distribution of work**: The Bank reserve the right to distribute the work for which quotation have been called, among more than one parties, if found necessary. No claim in this respect shall be considered and the contractor agrees to cooperate with other agencies appointed by the bank. |
|  |
| **Third party damage**: The contractor shall be responsible for all injury to persons, animals, building, building structure, any damage to road, streets, footpaths and shall rectify it at its own cost. |
|  |
| Insurance cover: All the workers of the contractor as well as his sub-contractor must be properly covered by an Insurance Policy under Workman’s Compensation Act and Fatal Accidents Act. The contractor at his own expenses arrange to effect and maintain until the virtual completion of the contract, insurance policy in the joint name of the Bank and the contractor against this risk to be retained by the Bank until the virtual completion of the work, and indemnify the Bank from all the liabilities arising out of such events. In case of delay, contractor shall arrange to extend insurance policy till work is completed. |
|  |
| **Delay & Extension of time**: All the work should be completed within the specified period in the tender. If the work is delayed due to the reasons beyond the control of the contractor, he should applying to the Bank explaining, therein the reasons for such delays, immediately and if in the opinion of Bank’s authorities the delay is justified, the contractor shall be granted extension in time limit. |
|  |
| **Certificate of virtual completion**: As soon as the work is completed, the contractor shall inform in writing such completion to the **PE department Regional office &** **Project Architect, M/s Mohit & Associates, L-2/554 Vineet Khand, Gomti Nagar Lucknow** who will inspect the work and if satisfied will issue the certificate that the work has been virtually completed and the defects liability period shall commence from the date of such certificate. |
|  |
| **Defect liability period**: The defects or other faults which may appear during the defect liability period which is 12 months after the virtual completion of the work, arising in the opinion of the bank due to inferior quality of material or bad workmanship not in accordance with the contract, contractor shall make good at his own cost within a reasonable time. In case of default, Bank may employ and pay other agencies to amend and make good such defects and all expenses / damages / losses shall be recoverable by Bank or may be deducted from any money due to the contractor |
|  |
| **Arrangement of work**: The contractor shall organize the work in such a way that the office users or the nearby public area put to no hardships and the working of the office is not affected. The contractor shall take adequate care during the progress of work to protect the office property like stationery, furniture, etc. In case of any damage, the same shall be made good by the contractor. Contractor is agreed to work after office hours for which no extra cost shall be considered. |
|  |
| **Stacking of material**: The contractor is not to stack any of his material recklessly so as to endanger the safety of the building and cause any nuisance to the occupants and the public. |
|  |
| **Extra charges**: It must be clearly understood that all the conditions of contracts are intended to be strictly enforced and that no extra charges in respect of extra work will be allowed unless they are clearly outside the spirit and meaning of the condition and unless such work shall have been ordered in writing. |
|  |
| **Protection of material and work**: The contractor shall be responsible for storing and watching his own material and protecting the work at his own cost. The contractor and his worker will be allowed to use lift after office hours. However, no paint drums or heavy bag of cement / paint will be allowed to be taken into the lift. Any damage / spoiling of lift / floor / dado caused during such act will have to be made good by the contractor at his own expenditure. |
| **Water supply**: The contractor shall make his own arrangement for water required for the work. in case the water is available and supplied by the Bank, the charges for the same shall be recovered at the rate of 1% of value of the work executed. In case water supplied by the Bank, the contractor shall make his own arrangement for the storage, pipeline from point of tape of to the required location. |
|  |
| **Electric supply**: The contractor shall make his own arrangement for Electricity required for the work. |
|  |
| **Approval of samples**: The contractor shall furnish well in time before work commence at his own cost, colour samples, samples of material or workmanship that may be called by Project Architect for approval. Rates quoted shall cover for such preliminary work. |
|  |
| **Workmanship**: The work involved calls for a high standard of workmanship combined with speed. All the glass panes, door handles / hinges, electric fitting, fans, furniture records, floors etc. are to be thoroughly cleaned after work is completed. Any damage to the flooring, tiles, dado, paneling or any other part of the building, etc. shall be made good at the cost of the contractor to the entire satisfaction of the Bank. Contractor shall make all arrangements for shifting of furniture / records and keeping the same in its original position after he finishes the work on daily basis. The contractor at his own cost shall provide brown paper, polythene, tarpaulin etc. for protecting furniture / fixtures, paneling, electrical, fittings, records, etc. |
|  |
| **Interpretation of documents / drawing**: Except where otherwise provided in the contract all questions and disputes relating to the meaning of the specifications, design drawings and instructions herein before mentioned and as to the quality of workmanship or materials used for the work or as to any other question, claim, right, matter or thing whatsoever, in any way arising out of or relating to the contract, designs, drawings specifications, estimates, instructions, orders or these conditions or otherwise concerning the works, or the execution or failure to execute the same whether arising during the progress of the work or after the completion or abandonment thereof shall be referred to the competent authority of the Bank whose decision shall be final and binding on the contractor. |
|  |
| **Use of scaffolding**: The contractor shall allow the use of scaffolding erected by them to any other agency employed by the Bank during the contract period without any payment. |
|  |
| **Provisional Item**: If ordered by the Bank, contractor shall be required to carry out provisional items at the same conditions and rates as applicable for this contract. |
|  |
| **Measurements of all concealed items**: Measurements of all concealed items of work and extra item if any, shall be got recorded by the Project Architect before they are checked up. |
|  |
| **Measurements**: All measurement tapes shall be of steel and all scaffolding and ladders that may be required for taking measurements shall be supplied by the contractor. |
|  |
| **Cleaning during the work**: The rates quoted shall include cleaning of ceiling roses, electric switches, boards, window panes etc. after the repairing leaving the site neat and tidy from time to time. |
| **Complying I.S. specification**: Unless otherwise mentioned in the contract, the latest Indian Standard Code for material specifications, method of work, and mode of measurements shall be followed. The payment shall be made on the basis of actual measurement of work done to be submitted along with bill |
|  |
| Rate to include: The rates quoted by the contractor shall cover for work at any height in the premises for all finished items under this contract. The rate quoted shall be inclusive of all material cost, wastage, labour, loading, profit, taxes if any, scaffolding, transport, supervision, spot light arrangement and any other means to complete the job. Octroi, sales-tax, works contract tax or any other taxes present or future to be included in the rates so quoted. |
|  |
| **Price Fluctuation**: The rates quoted by the contractor shall be firm throughout the currency of contract (including extension of time if any granted) and will not be subject to any fluctuation due to variation in the cost of material or labour |
|  |
| The successful tenderer if called upon to do so, shall obtain a letter from the approved trade manufacturer whose product is used, if found necessary by the Bank confirming that the manufacturer shall provide all the technical assistance and supervision during the execution of the work at all such places as directed and the contractor shall bear the expenses, if any, for such supervision and technical assistance supplied by the trade manufacturer. |
|  |
| **Testing of materials**: If at any point of time during the work, if Bank authorities desire to carry out the tests of certain materials, the contractor shall arrange for the same and submit the test report without any extra cost to the Bank. |
|  |
| The contractor shall note that they should bring to the notice of the PE department/Architect any breakage in glass window before starting work. However, if any glass window is found to be broken during the repairing work, the same shall be replaced by the contractor at his own cost. |
| **Conditional tenders:** Conditional tenders are liable to be rejected. |
|  |
| **Rates of non-tendered items**: The successful tenderer is bound to carry out any item of work necessary for the completion of the job even though such items are not included in schedule of quantities. |
| **Abandonment of work**: If in any case the work required to be abandoned, the contractor shall not be entitled for any claims and he will be paid as per the actual work done till that period. |
|  |
| The Bank reserves the right to accept / reject the lower or any or all tenders in part or in whole without assigning a reason therefor. |
|  |
| Decision of the Bank shall be final and binding on any matter connected with the work. The matter of any dispute shall be decided after mutual discussions based on the terms and conditions of this contract. However, if the matter can not be resolved then the same shall be referred to the respected, qualified person in the field agreed to both the parties and his opinion shall be binding on both the parties. However, this is precourse to any legal action in this regard. |
|  |
| **Incomplete quotation**: Incomplete quotations shall be summarily rejected |
| **Payments**: The contractor shall be paid by the Bank from time to time under interim payment on account of works executed and when the value of work equal to the approximate value named in the Appendix as ‘Value of work for Interim Certificate’ has been executed in accordance with this contract. |
|  |
| When the work has been virtually completed and Bank’s Architects / Engineer has certified in writing that the work has been completed on the basis of detailed measurements and has made a final scrutiny and that there is no dispute items, rates, ad quantities, the contractor shall be entitled to the payment of the final bill in accordance with the final certificate which will be honored within the period specified in the Appendix as period of honoring final certificate. |
|  |
| The contractor shall be paid by the Bank within the period named in Appendix (period of honoring certificate) after such certificate has been delivered to the employer by the Project Architect. Project Architect has power to withhold any certificate in the work or any part thereof are not carried out to his satisfaction or the contractor fails to show the desired progress or fails to follow the instructions given or in case of breach of this contract. |
|  |
| For water proofing works on traces, bathroom, WC, Chajja, work has to be executed through the agency specialized in waterproofing. Contractor will have to submit a guarantee of 10 years on stamp papers as per the format toe be prescribed by the Bank. |
|  |
| Earnest Money Deposit of successful tenderer shall be treated as security deposit with additional amount required to fulfill requirement of 5% of Tendered Amount (Inclusive of E.M.D.). The contractor should pay this amount to the Bank by DD or PO at the time of submission of tender. This amount shall be retained by the Bank till the work is virtually completed and all amounts relating thereto settled. Second part of security deposit shall be built through the retentions from interim and final bills of the contractor and the amount of retention shall be as stated in the Appendix. |
|  |
| When the certificate of the virtual completion is issued to the contractor the security deposit in the form Security Money shall be refunded, provided that the contractor has fulfilled all the conditions of contract and further provided that the employer has no claim for forfeiture of part or whole of the said deposit. The retention money built up through retention from interim and final bills will be returned to the contractor after the expiry of defect liability period, subject to deductions for any appropriations thereof required to be made by the Bank as per conditions of the contract. The contractor should note that no interest will be allowed on his security deposit. It will be minimum of 5% of Final verified Bill. |
|  |
| The contractor is requested to sign each page of the quotation and put rubber stamp, seal below his signature and seal the quotation in an envelope. |
|  |
| **Liquidated damages**: If the contractor fails to maintain the required progress or to complete the work and clear the site or before the contract or extended date period of completion, he shall without prejudice to any other right, pay as agreed compensation amount of **1** % of contract amount per week of delay subject to maximum of **10** % of contract amount as liquidated damages. |
|  |
| **Records & measurements:** Measurements shall be taken jointly by Project Architect and contractor and shall without extra charges provide assistance with appliance, labour and other things necessary for the work and measurements will be signed and dated by both the parties on completion of measurements. |
|  |
| **Safety measures:** The contractor at his own cost shall provide tarpaulins on the external side of the building at the time of breaking plaster etc. to safeguard adjacent property, Bank’s property, employees, traffic, etc. The contractor shall follow all the safety measures while carrying out the work. Employer that is Bank shall not be liable for any compensation due to accident, any mishap or negligence. |
|  |
| If there is delay in commencement of work for any reason, the employer that is Bank shall not be liable for any compensation. |
|  |
| If at any point of time during the progress, it is observed that the contractor is not progressing the work with due diligence, care and lagging much behind the schedule or fails to gear up the work despite instructions from Project Architect, the employer (Bank) reserves the right to terminate the contract with 7 days notice. In such case, the contractor shall be liable to pay the employer any extra cost involved for the completion of the said work and will not obstruct any way in completing the work through other agency. After completion of entire work the contractor shall be paid for the actual work executed by him at the quoted rates after deducting any claims, damages. In case of such termination the security deposit held by the Bank will be forfeited |
| Although the number of coats of paints / polishing / white washing are specified the contractor will have to additional coats if the surface is not to the satisfaction of the Project Architect and there shall be no extra payment on account of such coats |
|  |
| **First Aid:** The contractor shall be responsible for all first aid and he shall keep the site fully equipped to meet such emergency. |
| Supervision: The contractor is required to have on site during all working hours a competent supervisor (acceptable to Bank) who will be responsible for the conduct of worker and who has authority to receive and act on such instructions issued by the PE Department/Architect of Bank. |
|  |
| All work shall be carried out in a workman-like manner to the entire satisfaction of the Architect / PE Department. |
|  |
| Contractor shall follow all rules / regulations in force and should possess the license for employing labour and also follow all safety measures, labour bye law and shall be responsible for any lapse. |
|  |
| **Transfer of Tender Documents:** Transfer of tender documents purchased by one intending tenderer to another is not permissible. |
| **Safety:** The contractor shall carry out the entire work in a workman like manner having full regard for the safety of the men working at site. All safe practices shall be strictly adhered to by the workmen of the contractor like wearing helmets, safety belts when working at heights, gloves when handling sharp objects and reinforcement, eye shields during welding, safety shoes, etc. The contractor shall protect sides of openings in floor slabs, edges of slabs, stairs, stairwells etc. with barricades, warning signs / lights and educate all his workmen regarding following safe working practices. He shall provide first aid boxes at site. |
| In spite of following safe methods, in case of any unfortunate accident, the contractor shall indemnify the employer against any expenses or claims towards treatment or compensation. |
|  |
| **A Daily Diary Register:** A daily diary register (with cement and steel stock statement) will be kept in the Engineer’s Office or the site office. The contractor or his representative will furnish every day at 9.00 hrs. details of work for the day proceeding and the diary will be written up every day and jointly signed by the Engineer and the Contractor or their representatives in token of its correctness. |
|  |
| **Nuisance:** The contractor shall not any time do cause or permit anyone to do or cause any nuisance on the site or do anything which shall cause unnecessary disturbance of inconvenience to the Employer or to the owners, tenants or occupiers of other properties near the site and to the public generally. |
|  |
| **Rights, remedies and powers:** |
|  |
| I) Termination of contract due to contractor’s default. If the contractor: |
|  |
| 1. Abandonthe contract |
|  |
| b. At any time defaults in proceedings with the works with due diligence and continues to do so after a notice in writing of seven days from the Engineer or Project Architect or Employer, or |
|  |
| c. Commits default in complying with any of the terms and conditions of the contract and does not remedy it within **3RD days** after a notice in writing is given to him in that behalf of the Engineer or Project Architect or Employer. |
| d. Persistently disregards the instructions of the Engineer, Project Architect or contravenes any provision of the contract, or |
| e. Fails to remove materials from the site or to pull down and replace work after receiving from the Engineer, Project Architect notice to the effect that the said materials or works have been rejected. |
|  |
| f. Fails to complete the works or items of work on or before the stipulated date (s) of completion, and does not complete them within the period specified in a notice given in writing in that behalf by the Engineer, or Project Architect of Employer, or |
|  |
| g. Offer or gives or agrees to give to any person in the Employer’s service or to any other person on this behalf, any gift or consideration of any kind as an inducement or reward for doing or forbearing to do so for having done or forborne to do any act in relation to the obtaining or execution of this or any other contract for the Employer, or |
|  |
| h. Shall enter into a contract with the Employer in connection with which commission has been paid or agreed to be paid by him or to his knowledge, unless the particulars of any such commission and the terms of payment thereof have previously been disclosed in writing to the Employer / Engineer, or |
| i. Shall obtain a contract with the Employer as a result of ring tendering or other non-bonafide methods of competitive tendency, or |
|  |
| j. Being an individual, or if a firm, any partner thereof, shall at any time be adjudged insolvent or have a receiving order or order for administration of his estate made against him or shall take any proceedings for liquidation or composition (other than a voluntary liquidation fir the purpose of amalgamation or reconstruction) under any Insolvency Act for the time being in force or make any conveyance or assignment of his effects or composition or arrangement for the benefit of his creditors or support so to do, or any application be made under any Insolvency Act for the time being in force for the sequestration of his estates or if a trust deed be executed by him for benefit of his creditors, or |
|  |
| k. Being a company, shall pass a resolution or the court shall make an order for the liquidation of its affairs, or a appointed or circumstances shall arise which entitle the court or debenture holders to appoint a receiver or manager, or |
|  |
| l. Shall suffer an execution being levied on his goods and allow it to be continued for a period of 21 days, or |
|  |
| m. Assigns, transfers, sublets (engagement of labour on a piece work basis or of labour with materials not to be incorporated in the work, shall not be deemed to be sub-letting) or attempts to assign, transfer or sub-let the entire works, or any portion thereof without the prior written approval of the employer. |
|  |
| I) The Bank may, without prejudice to any other right or remedy which shall have accrued or shall accrue thereafter as the Employer by written notice determine the contract either as a whole or in part. |
|  |
| II) Upon such determination of the contract in whole or in part, the security deposit with the Employer in respect of the contract shall stand forfeited to the Employer without in any way effecting the rights of the Employer. |
|  |
| III) Rights of the employer after determination of the contract due to contractor’s default. |
|  |
| The Engineer shall on such determination have powers to: |
|  |
| a. Take possession of the site and any materials equipment, plant, implements stores etc. thereon, and / or |
| b. Carry out the incomplete work by any means at the risk and cost of the contractor. |
|  |
| IV) On determination of the contract in full or in part, the Engineer shall determine what amount, if any, is recoverable from the contractor for completion of the works or part of the works or in case the works or part of the works is not to be completed, the loss or damage suffered by the Employer. In determining the amount, credit shall be given to the contractor for the value of the work executed by him upto the time of cancellation or the value of contractor’s materials to be present so as to record the measurements in his presence. If the contractor fails to be present in response to the notice, the recording of measurements shall be proceeded with ex-parte and the measurements as recorded shall be binding the contractor. |
|  |
| V) The Bank shall have the right to use contractor’s plant, machinery and materials on the balance work but shall not in any way be responsible for any damage or loss of the same and the contractor shall not be entitled to any compensation thereof. |

# APPENDIX TO THE CONTRACT DOCUMENTS

**Subject : Interior Furnishing work for Baroda U.P. Bank at  MUSAFIRKHANA Branch,**

**Dist- AMETHI**

1. Defect liability period : **12 months** from the date of virtual

Completion of work.

2. Date of commencement : **3rd days** after the contract is accepted by

The contractor

3. Date of completion : **4** (**FOUR**) weeks.

4. Liquidated damages : 1% of contract amount per week / day of delay

Subject to maximum of 10% of contract amount

For the works of less than 6 month completion

Period.

5. Period of honoring final certificate : **45 days**

6. Period of honouring certificate : **15 days**

7. Security Money 5% of the tendered amount, will be sought as Security Money inclusive of EMD and will be released on completion of work.

8. Retention money 10% of the bill value will be deducted as retention subject to maximum security deposit. the retention money so held shall be refunded after defects liability period of 12 months of full & final completion of job.

9. Earnest Money to be submitted : **Rs. 5000/-** **(Rs. Five Thousand Only)**

by demand draft or pay order on any nationalised Bank drawn in favour **of Baroda U.P. Bank payable at GAURIGANJ AMETHI.**

**To,**

BARODA U.P. BANK

Regional Office AMETHI

Near Piyush Petrol Pump

Raebareli to Sultanpur Road

Gauriganj Amethi, 227409

Dear Sir,

**LETTER OF OFFER**

**Sub: Interior Furnishing works for Baroda U.P. Bank**

**at MUSAFIRKHANA Branch, Distt. AMETHI.**

With reference to the tender regarding the above work invited by you, we have to state as under.

We declare that before quoting the rates, we have visited the site and our rates are as per present site condition. Further we herewith deposit **Rs. 5000/- (Rs.Five Thousand Only)** as Earnest Money for due execution of the works at my /our tendered rates as per the Terms of Contract. In the event of this tender being accepted, I / We agree to enter in to and execute the necessary contract documents as required by you.

DD No.: Drawn on :

Dated : Amount :

As required by you, I / We are returning herewith the documents (in single) duly signed by us at each page in token of our acceptance of the provisions in the documents.

We hereby offer to execute and complete the whole of the works strictly in accordance with the said conditions of contract, special conditions of contract, specifications and drawings at the rates set out against each of the items of work in the schedule of quantities. the total cost included in the above is Rs.\_\_\_\_\_\_\_\_\_ /- (Rs.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ only).

We have carefully read and clearly understood the conditions of contracts, special conditions of contract, special conditions of contract and specifications. We agree to complete the work at the rate / rates quoted by me / us in the schedule of quantities and within the specified time from the date of work order awarding the work to us.

We understand the work is to be completed within scheduled time period.

Our rates are firm, include and cover all cost, expenses, liabilities of every description and all risk of every kind to be taken in execution and handing over the work to the Bank. The VAT, Service Tax, Sales Tax (State & Central), works contract tax, octroi, duties, municipal tax, general tax and any other taxes applicable and prevailing from time to time on such item for which the same are leviable and the rates quoted by us are inclusive of the same.

Thanking You,

Yours faithfully,

Name :

Address :

Tel. No. : (Fax. No.) :

Mobile No. :

**FORM OF AGREEMENT**

(On stamp paper of Rs.100/)

THIS AGREEMENT made this ……. Day of …………,2022……….. between Baroda U.P. Bank Near Piyush Petrol Pump Raebareli to Sultanpur Road Gauriganj Amethi, 227409.( hereinafter called “ the owner “ ) of one part and…………………………………………………………………………………………………………….………………………………………………………………… Of or whose registered office is situated at …………………..………………………………………………………………………………………………………………….……………………… ( hereinafter called : “ the Contractor “ ) of the other part.

WHEREAS the Owner is desirous of ……………………………………………………………………..…………………………………………………………………………… ……………. (hereinafter called “ the work “ ) at ………………………………………………………………………………...…………………………………………………………………………………………………………………………………………………

and has caused drawings and Bills of Quantities showing and describing the work to be done to be prepared by or under the direction of ………………………………………………………………………………………………………………………………………………………………………………………………………………………………….

AND WHEREAS the Contractor supplied the owner with a fully priced copy of the said Bills of Quantities ( which copy hereinafter referred to as “ the Contract Bills “ ) AND WHEREAS the said drawings ( hereinafter referred to as “ the Contract Drawings “) and The Contract Bills have been signed by on behalf of the parties hereto : AND WHEREAS the contractor has deposited the sum of Rupees……………………………………………………………….………………………………………………………………………………………………………………………. With the owner for due performance of this Agreement.

**NOW IS HEREBY AGREED AS FOLLOWS** :

For the consideration hereinafter mentioned the contractor will upon and subject to the conditions annexed carry out and complete the work shown upon the contract drawings and described by or referred to in the Contract Bills in the said conditions.

The Owner will pay the Contractor the sum of Rupees .............................................................….………………………………………………………………..……………………………………………………………………………….. ( hereinafter referred to as “ the Contract Sum “ ) or such other sum as shall become payable there under at the times and in the manner specified in the said conditions.

The term “ ARCHITECT “ in the said conditions shall mean the said  **M/S Mohit & ASSOCIATES, L-2/554 Vineet Khand, Gomti Nagar Lucknow** in the event of his death or ceasing to be the “ ARCHITECT “ for the purpose of this contract, such other person as the owner shall nominate for that purpose, not being a person to whom the contractor shall object for reasons considered to be sufficient by employer. Provided always that no person subsequently appointed to be the “ ARCHITECT “ under this contract shall be entitled to disregard or overrule any certificate or opinion or decision or approval or instruction given or expressed by earlier “ ARCHITECT “.

The said conditions there to shall be read and constructed as forming part of this agreement, and the parties hereto shall respectively abide by, submit themselves to the conditions and perform the agreements on their parts respectively in such conditions contained.

Any dispute arising out of the contract shall be referred to Arbitration as per the condition stipulated in clause of “ Special condition of contract “.

AS WITNESS the hands of the said parties.

Signed by the said OWNER

In the presence of witness

NAME:

ADDRESS:

Signed by the said CONTRACTOR

In the presence of witness

NAME:

ADDRESS:

**LIST OF FURNISHING MATERIAL**

|  |  |
| --- | --- |
| **PARTICULARS** | **Make of Material** |
|  |  |
| Plywood/Block Board | Archid / Century / Green  ( 6mm, 9mm, 12mm, 19mm) |
|  |  |
| Laminates | Greenlam / Century / Archid .  (1.0mm thick) |
|  |  |
| Soft Board (Pin up Board) | Jolly Board, Stylex |
|  |  |
| Gyp Board | India Gypsum/Armstrong/Gyproc |
|  |  |
| Metal Ceiling | Armstrong |
|  |  |
| Vertical Blinds | Vista, Universal, Maac |
|  |  |
| Screws | GKW / Mettle fold , Hindalco |
|  |  |
| SS Hinges | Godrej / Hardwyn |
|  |  |
| Hardware | Dorma, Hardwyn, Godrej |
|  |  |
| Drawer shutter lock | Godrej , Link, Dorset |
|  |  |
| Ball catch | Dorma, Hardwyn, Godrej |
|  |  |
| Door lock / Handles | Dorma, Hardwyn, Godrej |
|  |  |
| Veneer | Archid / Century / Green |
|  |  |
| Adhesives | Fevicol, Mahacol, Jeeevanjor |
|  |  |
| Wood Preservatives | Black Japan .. |
|  |  |
| Door closure | Dorma, Hardwyn, Godrej |
|  |  |
| Glass | Modi / Asahi / Saint Gobain |
|  |  |
| Glass tinted | Same as above. |
|  |  |
| Melamine Polish | Asian Paint, Nerolac . |
|  | French . Zinc oxide . |
|  |  |
| Paint | Burger, Nerolac, Asain |
|  |  |
| AC Grill | Air Products, Omicron, Patrawala |
|  |  |
| Vitrified tiles | Marbonite Jhonson, Kajaria |
|  |  |
| Ceramic Tiles | Jhonson & Jhonson, Kajaria, |
|  |  |
| Alu. Door & Window Sections | Jindal / Bhansail . |
|  |  |
| Floor springs | Dorma, Hardwyn, Godrej |
|  |  |
| Cement | ACC / Ambuja / Ultratech |
|  |  |
| White Cement | Birla Cement. JK Cement . |
|  |  |
| Sun Control film | Garware .. |
|  |  |
| Stainless steel sink | Nirali / Diamond .. |
|  |  |
| Carpet | Modi / Trans Asia/ Unitec |
|  |  |
| Rubber foam | 34 density mm foam |
|  |  |
| WC seat cover | Jaquor, Cera |
|  |  |
| Toilet paper holder | Dorma, Hardwyn, Godrej |

NOTE : All materials shall confirm to IS / BIS respective numbers.

* Commercial ply shall conform to IS 303.
* Marine Ply shall conform to IS 710
* Block Board shall conform to IS 1659.

**PREAMBLE TO BOQ**

**Abbreviations:**

|  |  |  |
| --- | --- | --- |
| R.M.T | : | Running Meter |
| Sq. Mt. | : | Square Meter |
| Sq. Ft. | : | Square Foot |
| Cu. Mt. | : | Cubic Meter |
| T.W. | : | Teak Wood |
| Q.R.O. | : | Quote Rate Only |
| C / C | : | Centre to Centre |
| M.T. | : | Metric Ton |
| C.P. | : | Chrome Plated |
| NO. | : | Numbers |
| MM | : | Millimeter |

1. All dimensions are in M.K.S. unless otherwise stated.
2. The quoted rate shall be all inclusive and cover the cost of material including wastage, freight, all types of taxes, duties, royalties, erection, construction, testing of materials if required samples brought for approval, tools and tackes, plant and equipments, supervision, overheads, profit and any other expenditure incurred for completion of work as per drawings, specifications and to the full satisfaction of BANK / Architect.
3. The rates quoted shall be valid for working at all heights, depths and on all floor levels. No extra payment shall be made for scaffolding, staging, ladders etc for transportation of men and materials at higher or lower levels.
4. The item rate specifications are indicative. the contractor will have to carry out the work in accordance with the drawings, technical specifications and / or other conditions laid down in tender document and to the full satisfaction of BANK / Architect.
5. Quantities mentioned against respective items are approximate and can varyto any extent. Payment shall be made on actually executed quantities.
6. No claims shall be entertained in case of increase / decrease quantities of any item and also to add / delete any item in totality. BANK / Architect reserve the right of operating any item for any work.
7. Rates for painting shall include cleaning glass panels, floors etc.
8. After completion of work the site shall be handed over absolutely clean, after ensuring that all floors, walls etc are spotlessly clean.
9. Rates of all items shall remain constant irrespective of floor level and nmo extra shall be paid for handling and stacking of materials, removing debris etc from the site.
10. Unless otherwise noted, the method of measurement will be as per I.S. 1200.
11. BANK / Architect reserve the right of operating all ' Quote Rate only ' items.
12. Wherever contractor proposes to use 'equivalent ‘makes (i.e. other than specified) he shall obtain BANK’s prior approval. BANK may ask Architect before giving approval to the same. Any additional cost and time lost due to this will be on Contractor's account and no claims will be entertained.
13. The rate of partition, paneling shall include necessary additional framework supports that may be required to suit site conditions or stability of the item. Decision of Architect in regards to the need for such additional supports shall be final.
14. All wooden frame work/ member size mentioned as out of, shall be full size with maximum planning tolerance of 3 mm both ways.
15. Rates for doors include all brass oxidized heavy duty hardware, locks, floor springs, door springs, door closer, special door handles etc as specified in relative terms.
16. Size and type of door closer/ floor spring shall be suitable for type of door. The contractor shall give guarantee for performance of door closer / floor spring from manufacturer.
17. Rates for partitions, paneling shall include making of necessary cut outs, chasing to be made for conduits, switch boards etc.
18. Rates for painting and polishing shall include cleaning glass panels, fans floor etc.
19. After completion of work the site shall be handed over absolutely clean, after ensuring that all laminates, floors walls etc are spotlessly clean.
20. Contractor shall clean the site and mark the lining out on the floor with adhesive tape for approval. The same shall not be paid separately.
21. In case of loose furniture, the specification for side unit or rear side credenza unit in any item shall be same as the specification of the table in that item.
22. All key hoes should be fixed with metallic key hole ring.
23. Key for all locks should be different and no key should match with two different locks.
24. Rates shall include for following:-

PLASTERING:

* 1. Work at all levels, heights and in all situations and profiles.
  2. Double scaffolding, working platforms / Tarpaulin curtains.
  3. Coving, drip moulds, grooves, recesses, ornamental bands etc.
  4. A coat of white wash for neeru plaster soon after curing period is over.
  5. Work in narrow width and small quantities unless special provision is made to the contrary.
  6. Preparation of surface by ranking out joints in brick or by hacking the concrete surface and wetting the surface before plastering wherever required.
  7. Thickness of plaster exclusive of the thickness of key i.e. grooves and open joints in brick work, stone work etc.
  8. Chambers of any width, internal and external rounded angle.
  9. Curling, protection and cleaning of all surfaces.
  10. Keeping all plastered surfaces well wetted for at least 7 days.

PAINTING & POLISHING:

1. Works at all heights and use of all scaffolding, necessary for execution of work and for inspection.
2. Preparing surfaces to receive finishing coats.
3. Putting sand papering and dusting of surface in between coats where applicable.
4. Work on cornices, narrow bands and widths, grooves etc.
5. Finishing to approved matt textures, complete as directed.
6. Spreading and removing, covering to doors, windows, floors, fittings etc to protect them from splashes.
7. Washing floors, cleaning glass, joinery, electric fittings etc and leaving premises clean and tidy.
8. Mode of Measurement

|  |  |  |  |
| --- | --- | --- | --- |
| S.No. | Particulars | Method of Measurement | Multiplying Factors |
| 1 | Panelled doors & Windows | Measured flat not girthed including frame | 1.125 for each side |
| 2 | Fully glazed | 0.5 for each side |
| 3 | Partly glazed & panelled | 1.0 for each side |
| 4 | Flush door | 1.0 for each side |
| 5 | M.S.Grill & Collapsible door | 1.0 for painting all over |
| 6 | Rolling Shutter | Measured flat not girthed including frame | 1.25 for each side |

**Mode of Measurements:**

|  |  |  |  |
| --- | --- | --- | --- |
| 1 | Partition, Paneling | : | Sq. Ft. Area - one side only |
| 2 | Painting | : | Sq. Ft. Finished area only |
| 3 | Rounding off Measurements | : | All measurements shall be rounded off to nearest 2 decimal points. |

**Summary**

**BARODA U.P. BANK**

**MUSAFIRKHANA BRANCH DISTT. RAE BARELI**

|  |  |  |  |
| --- | --- | --- | --- |
| **sno** | **Description** | **Section** | **Amount of Tender** |
| 1. | Furnishing works | in digits |  |
|  |  | in words |  |
|  | TOTAL | in Digits |  |
|  |  | In words |  |
|  | GST 18% | In words |  |
|  | GRAND TOTAL | in Digits |  |
|  |  | In words |  |

Note :-

1. All materials to be used strictly follow the list of approved materials.
2. Any deviation in the use of materials at site other than approved materials list will not be permitted and the bank may cancel the contract at any time for any such misconduct & colour as per bran manual.
3. The workman ship and quality of work should be of good quality and to be satisfaction level of the bank’s architect and bank

TENDER OF FURNISHING WORKS FOR ***BARODA U. P. BANK*** SITUATED AT MUSAFIRKHANA BRANCH DISTT.Amethi.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | |  | | --- | |  | |  |  |  |  |
| **B.O.Q OF FURNISHING WORK BARODA UP BANK BRANCH AT MUSHAFIRKHANA,AMETHI(UP)** | | | | | |
| **A** | **SCHEDULE - 'A' (FURNISHING WORK)** |  | | | |
| **S.NO.** | **DESCRIPTION** | **UNIT** | **QTY.** | **RATE** | **AMOUNT** |
| **1** | **PARTITIONS WORK** |  |  |  |  |
| **1.1** | **FULL / LOW HEIGHT SOLID PARTITION / DOOR /UPS** | Sq.Ft. | 65.00 |  |  |
|  | Full ht. Solid Partition up to ceiling only WITH LOUVRE :- Providing and fixing solid partition , the framing shall made out of aluminium hollow section of 65mm x 37mm size 1.5mm thick of JINDAL / INDAL as internal frame structure placed horizontally & vertically at max distance of 2’-0” x 2'-0" center to center. Fixing 6 mm thick commercial ply on both sides with 1.0mm thick laminate on top of approved shade with groove pattern as per instructions of Architect. The rate shall include the cost of providing skirting of 100mm wide lined with 1mm thk laminate and providing & fixing a border at top of 100mm wide lined with 1mm thk laminate complete. Laminate Should be considered up to two or three color combination. The edge beadings with steam beach wood should be finished with melamine polish if required, frame work above false ceiling done shall not be measured but contractor may factor it while quoting there rates as measurment up to false ceiling lvl.. |  |  |  |  |
|  | The rate inclusive of providing & fixing of required flush door of 37mm thick approx. with 1.0mm th.laminate both side with steem beech wood chowkhat of size 75mm x 65mm approx and Item includes Heavy-duty SS ball bearing butt hinges 100 x 5.5 mm (4 Nos. per shutter) with screws etc.The shade of laminate finish to be got approved from Bank. . All as per the design and instructions Bank. |  |  |  |  |
|  | Note :- For the purpose of payment partition shall be measured including the area of door/door frames up to false ceiling heaight. |  |  |  |  |
|  | Framework shall be regidly secured to floor, bottom of slab & exisitng walls at 2'-0" c/c with dash fasteners. |  |  |  |  |
| **1.2** | **7' Height Glazed partition in Cash cabin** | Sq.Ft. | 140.00 |  |  |
|  | Same as of Solid ht. partition , providing Aluminium grill jalli above 1'-0" / 3'-0" & up to 7'-0" fixed with steam beech wood beading of finished size 1 1/2" X 1" all along the edge. All exposed woodwork to be mealamine polished. All as per the design and instruction Bank. |  |  |  |  |
| **1.3** | **4.5' Height Semi Glazed Partition manager cabin / Counter** | Sq.Ft. | 250.00 |  |  |
|  | Same as above but of Low height as per design including 10mm Toughened glass with edges polished to be used. All other specs are same as of above, Edges of the partition to be covered with 3" X 1.5" Steam beech wood duly melmine polished moulding. 38mm thick flush door: **wicket gate** also shall be included for a measurement. All as per the design and insturction bank. |  |  |  |  |
| **1.4** | **Front Glazeing cash cabin** | Sq.Ft. | 20.00 |  |  |
|  | Providing & fixing 10mm thick toughened clear float glass to shape for front side of the cash counters including cutting the holes and providing & fixing TW beading polished and tinted to approved shade. ( including SWO/Chief Cashier front Glass). |  |  |  |  |
| **1.5** | **Aluminium grill on the ceiling of Cash cabin** | Sq.Ft. | 35.00 |  |  |
| **2** | **DOOR & ACCESSORIES** |  |  |  |  |
|  |  |  |  |  |  |
| **2.1** | **Main Entrance Door with Fixed Glazing powder coated** | Sq.Ft. | 0.00 |  |  |
|  | Providing and fixing Powder coated aluminium entrance doors with 12mm floatglass (3M frosted sticker) as/design with top & bottom section of 45 by 90mm , 2mm thick section of hindalco/indal anodized in approved colour with 25 micron anodizing along with SS C shaped handles of kitch or equivalent make along with floor spring of hemco/everite make. The item also includes door lock completed to the satisfaction of the architect. |  |  |  |  |
|  |  |  |  |  |  |
| **2.2** | Supplying and fixing of Dorma/GEZE Dline / Hardwyn/Godrej or approved equivalent Door Closer for wooden door for Cashier . | Nos | 1.00 |  |  |
| **2.3** | Supplying and fixing of mortice door lock of hardwyn make HML-480 Lock Body 304 Stainless Stell. (in BM Cabin , Store room 0. Cash cabin shall be Godrej Night latch. | Nos | 1.00 |  |  |
| **2.4** | Supplying and fixing of door stopper SS Grade 304, HESSF-2C hardwyn make. | Nos | 5.00 |  |  |
|  |  |  |  |  |  |
| **3** | **WORKING COUNTER** |  |  |  |  |
|  |  |  |  |  |  |
| **3.1** | **CASH COUNTERS** | Rft. | 5.00 |  |  |
|  | Providing and fixing Chief Cash Counter in split-levels @ 2’-6” (height 750mm) & 18” (1140mm) with 2’-6” & 15” wide each respectively . Upper levels having shall be finished with 1.0mm thick laminate of approved shade and colour with approved adhesive to 19 mm thick commercial ply top. Edges of 18” wide counter shall be finished with 1.0mm thick laminate of approved shade and colour. Lower tier shall be made of 19 mm thick ply wood finished in 1.5mm thick laminate. Exposed edge having steam beech wood edging of size 1 ½” x 1”. Vertical face shall have 19mm thick ply wood over pine wood framework as per requirement of design. All exposed surfaces shall be finished with 1.0mm thick laminate of approved shade and colour. |  |  |  |  |
|  | 1 no. prefabricated metal computer key board tray including drawer slides 12.5” x 22” tray with 14” telescopic slides including L – brackets for securing to the table top. Chest of drawers (size 1’-4” x 2’-0” x 2’- 5”) made of 19mm thick commercial ply wood having three drawers finished with 1.0mm thick Laminate on all sides. Each drawer shall have locking system and 6” long S.S. brushed finished handle, drawer slides etc. of approved make. All exposed edges of ply wood sealed with Steam beech wood beading of size ¼” x ¾”. All beading and exposed wood shall be melamine polished and non-laminate surface to be enamel painted. Item includes readymade metal powder coated CPU trolley, grommet, footrest for each seat. All complete as per approval and instructions of the Architect / employer.The rate also include providing and fixing painting a foot rest using hard wood 100 x 25mm size 1st class seasoned country frame. |  |  |  |  |
|  | Payment will be made only on the centerline measurement. The rate shall include the cost of providing skirting of 100mm wide lined with 1.0mm thk laminate and providing & fixing a border at top of 100mm wide lined with 1.0mm thk laminate comlpete. |  |  |  |  |
|  |  |  |  |  |  |
| **3.2** | **RUNNING COUNTER** | Rft. | 9.50 |  |  |
|  | Providing and fixing staff counter/SWO @ 2’-6” (750 mm) shall be made of 19mm thick ply wood and finished in 1 mm thick laminate. Working top having steam beech wood edging of size 1 ½” x 1”. Vertical face shall have 19 mm thick commercial ply over pine wood framework as per requirement of design. All exposed edges of ply wood sealed with Steam beech wood beading of size ¼” x ¾”. All exposed surfaces shall be finished with 1.0mm thick laminate of approved shade. |  |  |  |  |
|  | The item includes Chest of drawers (size 1’-4” x 2’-0” x 2’- 5”) made of 19mm thick commercial ply wood having One drawers at top and a storage cabinet below having shutters of 19mm thick ply wood finished with 1.0mm thick Laminate on all sides. 1 no. prefabricated metal computer key board tray including drawer slides 12.5” x 22” tray with 14” telescopic slides including L – brackets for securing to the table top for each seat. All beading and exposed wood shall be melamine polished and non-laminate surface to be enamel painted. Item includes 1’-3” high 12mm thick toughned glass above upper tier and readymade metal powder coated CPU trolley, grommet, foot rest for each seat. All complete as per approval and instructions of the Architect / employer.The rate also include providing and fixing painting a foot rest using hard wood 100 x 25mm size 1st class seasoned country frame. Payment will be made only on the centerline measurement. |  |  |  |  |
|  | The rate shall include the cost of providing skirting of 100mm wide lined with 1.0mm thk laminate and providing & fixing a border at top of 100mm wide lined with 1.0mm thk laminate comlpete. |  |  |  |  |
|  |  |  |  |  |  |
| **4** | **TABLE & FURNITURE** |  |  |  |  |
|  |  |  |  |  |  |
| **4.1** | **MANAGER TABLE ( Size:- 6'-0" x 2'-6") ht. 2'-6"** | Nos | 1.00 |  |  |
|  | Providing and fixing tables made out of 19 mm thick commercial ply over hard wood frame work finished with 1.5mm thick laminate of approved shade. Top having steam beech wood edging of size 2” x 1 ¾”. 10mm thick clear float glass with beveled edges shall be provided on the finished to 19mm thk Comm.ply wood of approved make cladded with 1mm thk. laminate( color with vertical grain) as per design in all visible areas. All the exposed edges to be covered with wooden steam beech lippings and mouldings duly malamine polish. The drawers to be made out of 19mm thk ply wood with 1.0 mm laminate finish in the front , and bottom to be made out of 6mm plywood and it should play in drawer sliding telescopic channels. The inside of the drawer to be duly paint & Table back side wil be 1mm laminate. A leg rest to be provided duly polished made out of 3"x2" Wooden Section. |  |  |  |  |
|  | A shutter to be made by 19mm ply wood cladded with1.0mm laminate .The necessary locks handles to be provided in each drawers and shutters. 3" x 1/2" wooden skiritng to be provided in all visible areas duly polished. The necessary wire managers(SS) to be provided on the tables and provision for lights to be kept if required in the front of the table. All the exposed areas to be duly malamine polished The work to be completed as per design and approval of the Bank. The table should have key board tray and CPU Trolly to be Modular. All as per the design and instructions Bank . |  |  |  |  |
| **4.2** | **OFFICER TABLE WITHOUT GLASS ( Size:- 5'-0" x 2'-6") ht. 2'-6"** | Nos | 1.00 |  |  |
| **5** | **STORAGE & SIDE UNIT** |  |  |  |  |
|  |  |  |  |  |  |
| **5.1** | **Side Unit** |  |  |  |  |
|  | Providing and fixing Side Unit/ Back unit 400 mm depth made out of 19mm ply wood finished with 1.0mm laminate in all exposed areas and top shall be 1.5 mm thick . The drawers to be made out of 19mm commercial plywood and cladded with 1.0mm laminate and bottom made out of 6mm comm ply duly painted in matching tone and it should play on drawer sliding channels . The shutters to be made out of 19mm commercial ply wood and should play on drawer sliding castors on powder coated channels. The necessary locks , handles, etc to be provided . 3" x1/2 wooden skirting to be provided duly polished as per matching tone all along the visible areas . Inside of the unit to be enamel painted in matching tone . All the exposed edges of the boards/ply woods to be coverd with woden lippings/mouldings duly polished all complete. The work to be completed as per approval and specification of the Architect. | NO | 2.00 |  |  |
| **5.2** | **2.5 feet height Storage** | Sq.Ft. | 30.00 |  |  |
|  | Providing and fixing Full /Low height Cabiner 1'-9" mm deep made out of 19mm thk plywood finished with 1.0mm laminate in all exposed areas . The Shutter to be made out of 19mm ply wood in the front cladded with 1.0mm laminate( color, vertical grain) . and bottom made out of 6mm plywood duly painted in matching tone and shelves 19mm thk comm ply wood to fixed inside storage. The shutters to be made out of 19mm ply wood . The necessary locks , handles, etc to be provided . 3" x1/2 wooden skiritng to be provided duly polished as per matching tone all along the visible areas . Inside of the unit to be enamel paint finish . All the exposed edeges of the boards/plywoods to be coverd with wooden lippings/mouldings duly polished all complete.All as per the design and instructions Bank. |  |  |  |  |
| **6** | **OTHER MISCELLANEOUS ITEMS** |  |  |  |  |
|  |  |  |  |  |  |
| **6.1** | **PIN UP / NOTICE BOARD** |  |  |  |  |
|  | Providing and fixing soft board with necessary framework with 12mm BWR plywood on top 12 jolly board to be fixed finished with fabric @Rs80 , with necessary mouldings duly polished along the periferi. All as per the design and instructions Bank. | NO | 1.00 |  |  |
|  |  |  |  |  |  |
| **6.2** | **WRITING LEDGER & Cheque & sugestion box** | NO | 1.00 |  |  |
|  | Providing and fixing writing ledge as per design minium 5 ft length made out 19mm comm. board with necessary grove patterns with 1.0mm laminate. 10mm thk machine polished glass to be provided on top of the writing ledge. Small boxes to be made out of 12mm comm. ply to be made on top of the writing ledge finished with 1.0 mm laminate, inside enamel painted and rate should be included providing fixing of sugestion box & Cheque deposit box as per approval of bank .The work to be completed as per design and approval of the architect. |  |  |  |  |
| 6.3 | **Main Electrical Panel Cabinet** |  |  |  |  |
|  | Providing and fixing of DB Shuttering formed of 12mm thk plywood wood on 12mm thick Gypsum board (fire Proof) with finsih as per Item no 1 for inside and out side shutters finished with laminate on outer surface with SS (4Nos) louvre perforation and necessary hardware,hinges etc complete as per details. All as per the design and instructions Bank. | Sq.Ft. | 40.00 |  |  |
| **6.4** | **Shutter boxing for ROLLING SHUTTER** |  |  |  |  |
|  | P & F shutter boxing made of 19 m.m. phenol bonded ply IS 303 grade including hatch fir pulling down & up the rolling shutter.The box to be laminated with aluminium composite panel of 3.0 m.m. completed to the satisfaction of architect.Front surface will be taken for measurement only. | Sq.Ft. | 60.00 |  |  |
| **6.4** | **PILLAR WOODEN PANELLING** | Sq.Ft. | 70.00 |  |  |
|  | Fabricating and fixing wall/column paneling, the framing shall made out of aluminium hollow section of 65mm x 37mm size 1.5mm thick of JINDAL / INDAL at spacing not exceeding 600mm bothways (horizontal and vertical). Paneling framework to be secured to wall surface/column surface.Paneling framework to be clad on one side with 9mm thick ply finished with 1.0mm thk laminate including skirting of 100mm high & 12mm x 12mm groove at skirting level. All as per the design and instructions Bank. |  |  |  |  |
| 6.5 | **Customer Table - (4'-0" X 2'-6" )** | No | 1.00 |  |  |
|  | Providing and making a table of over all size of top as mentioned above. It shall consist of ¾” thk. Comm. Ply top as per design (double edge on outer edge with 1 1/2" thk half moulding on the edges) supported on ¾” thk. Comm. Ply verticals.supported on wooden base (as designed by the architect). Suitable wooden moulding as architect design with mellamine shall be provided to the edge of the top. All external surfaces to be finished in 1 mm laminate. |  |  |  |  |
|  | **GRAND TOTAL FOR FURNISHING (A)** |  |  |  |  |
|  |  |  |  |  |  |
|  | **\* GST EXTRA AS APPLICABLE** |  |  |  |  |